1. WIRELESS MIC RECEIVER

모델 : MYFIX, HW-920R

(1) 기  능

본 기기는 2채널 무선마이크용 수신기로써, 끊김 없는 다이버시티 수신 시스템이 적용되어 있으며, 각 채널에는 주파수 채널링을 완전히 제거하기 위해 독립적인 ID 코드가 제공되며, IR버튼으로 편리한 송수신 세팅이 가능하며, 송수신 거리 조절 기능이 탑재된 기기로 다음의 성능 이상이어야 한다.

(2) 성  능

[Receiver]

- Frequency range : 925.0 ~ 937.5MHz

- Number of adjustable channels : 3000X2

- Frequency stability : 0.002PPM

- Receiving sensitivity : -100dB

- Tone frequency response : 60hz-18khz (3dB)

- Harmonic distortion : < 0.5%

- Signal to noise ratio : ＞105dB

- Dynamic range : 105dB

- Maximum frequency offset : ±48KHz

- Stray suppression : ≥75dB

- Audio output : balanced output and unbalanced output

- Power supply : 12-18V DC/1000mA

[Hand MIC]

- Frequency range : 925.0 ~ 937.5MHz

- Number of adjustable channels : 3000X2

- Frequency stability : 0.002PPM

- Receiving sensitivity : -100dB

- Tone frequency response : 60hz-18khz (3dB)

- Harmonic distortion : < 0.5%

- Signal to noise ratio : ＞105dB

- Dynamic range : 105dB

- Maximum frequency offset : ±48KHz

- Stray suppression : ≥75dB

- Audio output : balanced output and unbalanced output

- Power supply : 12-18V DC/1000mA

- 동등 또는 이상 품이어야 한다.